Safe Work Method Statement (SWMS)
Template for high risk construction work - complies with the WHS Regulation requirements for SWMS content. Complete every section before work starts, consult the workers involved, and keep the SWMS available on site.
1. Project and PCBU details
	Field
	Details

	Company / PCBU name
	

	ABN
	

	Principal contractor
	

	Project / site address
	

	Work activity covered by this SWMS
	

	SWMS prepared by (name, position)
	

	Date prepared
	

	Date of last review
	



2. High risk construction work involved
Tick each class of high risk construction work under WHS Regulation 291 that applies, e.g. work at height above 2 m, work near energised electrical installations, work in or near a trench deeper than 1.5 m, tilt-up or precast concrete, demolition, asbestos disturbance, work near mobile plant, work over or near water.
3. Job steps, hazards and controls
	Job step
	Potential hazards
	Risk rating (H/M/L)
	Control measures (hierarchy of controls)
	Person responsible

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



4. Plant, equipment and PPE
	Plant / equipment used
	Inspection or licence requirement
	PPE required

	
	
	

	
	
	

	
	
	



5. Worker consultation and sign-off
Each worker carrying out the work must be consulted on this SWMS, understand the controls, and sign below before starting work.
	Worker name
	Signature
	Date

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



Review triggers: review this SWMS whenever the work, the workplace, or the controls change, after any incident or near miss, and at the dates scheduled above.
Template provided free by Pulsify (pulsify.tech). Not legal advice - confirm requirements with your state WHS regulator.
